# 1. Configure the DMZ with iptables

Objective: Configure a Demilitarized Zone (DMZ) on a Raspberry Pi using iptables to route and secure network traffic.

## Commands:

sudo iptables -t nat -A PREROUTING -p tcp --dport 80 -j DNAT --to-destination 192.168.50.10:80  
sudo iptables -t nat -A POSTROUTING -j MASQUERADE

## Comments:

- This configuration redirects all HTTP traffic to the internal IP 192.168.50.10.  
- MASQUERADE ensures that the traffic is anonymized when it exits the network.

## Importance:

5/5